{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["5万以上"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"5万以上","index":0,"n_rows":47,"n_cols":9,"rows_kept":47,"merged":[[0,0,0,6]],"flags":["formulas_cached_only"]}
["台州市中医院医疗设备拟采购计划及预算"]
["序号","类别","设备名称","数量","主要配置和参数要求","预算金额(总价)（万元）","科室"]
[1,"G","康复评估训练系统",1,"标配，移动显示系统、软件、无线传感器；具有Gait Watch三维步态分析与评估系统；Flex Table 数字OT评估与训练系统；Bio Flex 上肢运动控制评估与训练系统；Bio Flex姿势控制评估与训练系统；Bio Mastetr 虚拟情景互动评估与训练系统",106,"康复科"]
[2,"G","吞咽言语诊治仪",1,"主机一套，标配；具备言语发音治疗软件、音箱、MP3机等",16.8,"康复科"]
[3,"G","等速肌力训练系统(3.5/个)","1套（8件）","标配，具备高硬度刚体结构；10档双向阻力调节",28,"康复科"]
[4,"G","JAS可调式固定支具(5/个)","1套（8件）","固定支具；可应用于各关节手术后的早期康复治疗",40,"康复科"]
[5,"G","深层肌肉刺激仪（DMS）",1,"主机一套，标配，手持式，具有三种钛合金治疗头：20mm、25mm、35mm，治疗头振动频率为60Hz、振幅≥6mm；重量≤3KG，具有多种支点式手持方式，",5,"康复科"]
[6,"G","经颅直流电刺激仪（tdcs）",1,"主机一套，标配；具有CES和tDCS两种刺激模式；CES模式治疗时间：0-60min可调，满足临床治疗及科研需求；",40,"康复科"]
[7,"G","磁场刺激仪",1," 主机一套，标配，刺激频率：0-100Hz可调；刺激线圈能实现双面双向刺激，最大刺激强度6Tesla，且0-6Tesla连续可调",68,"康复科"]
[8,"G","多点多轴悬吊系统",1,"标配，≥7个悬吊点，方便治疗患者多个部位；质量极佳，永久耐锈，承重量≥1500kg；专业康复治疗系统，多种固定支架可选；操作简易",25,"康复科"]
[9,"A","便携肌骨超声",1,"主机一套，标配；腹部探头频率1~8兆赫，高频探头频率6~18兆赫",60,"康复科"]
[10,"G","盆底肌生物反馈电刺激仪",1,"主机一套，具有全方位多功能的盆底综合治疗系统（生物反馈系统、电刺激系统、尿流率系统、2个肌电图系统、压力测定系统）",20,"康复科"]
[11,"G","肉毒素注射引导仪",1,"配肌电声音反馈仪1台，专用刺激针电极1套，手持式，具有LCD屏幕显示肌电波形、EMG声音提示、RMS、IEMG数据分析，肌电图结合电刺激双重引导药物治疗；",8,"康复科"]
[12,"G","体外冲击波治疗系统",1,"主机一台，标配",40,"骨一科"]
[13,"D","关节镜摄像系统",1,"主机一套、高温高压摄像头、光纤导线、4MM30度关节镜、闭孔器、进水开关等",50,"骨一科"]
[14,"F","乳房活检及旋切系统",1,"主机一台，旋切刀头（耗材）",35,"普外科"]
[15,"F","手术动力装置",1,"配备电机、控制箱、颅骨钻、颅骨铣刀及高速磨钻；具有转速高、质量稳定",15,"神经外科"]
[16,"F","手术显微镜",1,"标配，助手镜、折叠式双目镜筒、摄录像系统",70,"神经外科"]
[17,"F","手术灯",2,"标配，led无影灯，使用方便、耐用",16,"手术室"]
[18,"F","电动手术床",1,"标配，低体位，一腱复位，能跟原先的牵引床匹配",20,"手术室"]
[19,"E","麻醉机(含监护）",2,"标配，麻醉深度，IBP，CVP监测，呼吸容量环监测",90,"麻醉科"]
[20,"G","自体血回输机",1,"主机 1台，承载车 1辆，挂架 1套",15,"麻醉科"]
[21,"F","VIO电外科工作站",1,"自检系统、过载保护、功率智能控制系统、能量初始系统、脚踏开关无线远程控制等，可与超声刀等手术设备配套使用",15,"消化科"]
[22,"G","全自动染色机",1,"标准配置.双层，两组染色程序同时进行，用于组织切片及细胞学染色",22,"病理科",null,22]
[23,"G","全自动封片机",1,"主机一台，标配",20,"病理科",null,20]
[24,"G","肺功能仪",1,"主机一台，标配",6,"健康管理中心"]
[25,"G","生物刺激反馈仪",1,"主机及全套附件，双通道、电刺激，适用于产后盆底康复、尿失禁、盆底术后功能重建（评估版）",7.5,"健康管理中心"]
[26,"B","全自动血流度测试仪（血流变）",1,"标配",6.5,"检验科"]
[27,"B","发光免疫",1,"标配",5,"检验科"]
[28,"B","全自动细菌鉴定药敏分析仪",1,"标配，梅里埃VITEK 2—compact，细菌监测、分析",35,"检验科"]
[29,"B","全自动精液分析仪",1,"主机一台，图文工作站，标配",8,"检验科"]
[30,"B","研究级显微镜",1,"显微镜、电脑、分析软件",6.2,"检验科"]
[31,"B","白带常规分析系统",1,"标配，",8,"检验科"]
[32,"B","二氧化碳培养箱",1,"标配，",5,"检验科"]
[33,"G","连体式牙科综合治疗机",2,"标配，治疗椅,冷光灯，陶瓷痰盂缸，净水系统，三用枪（高、低速手机、医生椅、上挂式）",8,"口腔科"]
[34,"E","监护仪(抗震）",2,"标配，具有抗震、防摔功能",9.6,"急诊科"]
[35,"G","可视喉镜",1,"标准配置.满足抽吸、钳取、给药、给氧、插管等需求；软管前端可弯曲",8,"急诊科"]
[36,"B","血气分析仪",1,"主机一套，检测参数：CO2、O2、PH、HCO3、K+、NA+",10,"ICU"]
[37,"G","床边血液净化（CRRT）",1,"床边血液净化；管路和滤器分离，可自由选择滤器。",24,"ICU"]
[38,"E","有创呼吸机",3,"主机、台车和空压机；呼吸模式：SIMV、PRVC、PC",60,"ICU"]
[39,"E","无创呼吸机",1,"主机、台车 模式：S/T、PCV、AVPAPS",16,"ICU"]
[40,"G","高压注射器",1,"配套西门子16排CT",30,"放射科"]
[41,"D","电子胆道镜及配套器械",1,"主机及全套附件，图像清晰，能与医院现有设备兼容互换使用",30,"普外科"]
[42,"D","电子（纤维）支气管镜",1,"主机及全套附件，内置高清晰度CCD、变焦功能扩大画面尺寸,可利用带水囊的超声波探头进行EBUS\n ",50,"呼吸科"]
[43,"G","血透机",1,"标配、血液透析（HD）功能、报警功能",16,"血透室"]
[44,"G","颈腰椎牵引器",1,"标配",4,"康复科"]
[45,"G","高频电刀",1,"标配",4,"妇产科"]