{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["台州市中医院医疗设备拟采购计划及预算"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"台州市中医院医疗设备拟采购计划及预算","index":0,"n_rows":35,"n_cols":9,"rows_kept":35,"merged":[[0,0,0,6]],"flags":["formulas_cached_only"]}
["台州市中医院医疗设备拟采购计划及预算"]
["序号","类别","设备名称","数量","主要配置和参数要求","预算金额(总价)（万元）","科室"]
[1,"G","全自动冰点渗透压计",1,"主要是针对测量血浆或血清，尿液，粪便等的渗透压进行测定。",6,"检验科"]
[2,"G","全自动血沉仪",1,"主机、电源装置、条形码阅读器、混合器、打印机、血沉管、软件及其它附件组成。临床上用于测定红细胞沉降率。",22,"检验科"]
[3,"G","血浆融浆机",1,"也成血液融浆机，血库的配套器具，对低温血浆溶化减少了工序，节省时间。",1,"检验科"]
[4,"G","显微镜",1,"普通光学显微镜，标准配置",1,"检验科"]
[5,"G","飞行时间质谱仪",1,"主机、有进样系统、分析模式、谱图、数据处理系统等",150,"检验科"]
[6,"G","药柜",10,"标准配置",8,"药剂科"]
[7,"G","运药车",2,"标准配置",2,"药剂科"]
[8,"G","便携式冷藏箱",2,"标准配置",6,"药剂科"]
[9,"A","单剂量分包机",1,"实现药品分类、分配、包药、打印、封装及对药品的存储管理功能",120,"药剂科"]
[10,"G","医用冰箱",1,"标准配置",3,"中药房"]
[11,"G","心肺复苏仪",1,"也称作心肺复苏机，心肺复苏器等，是用于救治心跳骤停的机械设备",30,"急诊"]
[12,"G","医用控温毯",1,"标准配置",5,"急诊"]
[13,"D","血透机",1,"普通型",15,"血透室"]
[14,"F","血透机",1,"超滤型",25,"血透室"]
[15,"F","床边超声",1,null,25,"ICU"]
[16,"F","无创呼吸机",1,"主机、台车 模式：S/T、PCV、AVPAPS",18,"ICU"]
[17,"F","有创呼吸机",4,"主机、台车和空压机；呼吸模式：SIMV、PRVC、PC",52,"ICU"]
[18,"F","转运呼吸机",1,"适用于潮气量大于50mL的患者的急救以及运转时对病人的人工通气。一体化气路设计，使用简单快捷，适合在多种场合使用。",6,"ICU"]
[19,"E","营养泵",1,"标准配置",5,"ICU"]
[20,"G","转运床",1,"标准配置",1,"手术室"]
[21,"F","儿童床",20,"适用儿童患者的病床",10,"儿科"]
[null,null,"儿童呼吸机",1,"适用于婴幼儿和体重20KG的小儿，配备多种适用于新生儿患者的呼吸模式，先进的比例辅助通气和血氧饱和度控制的后备通气模式， 比例阀式控制系统，吸气/呼气端协同控制，先进的低死腔量流量传感器系统，内置湿化系统提供充分的分子式湿化效果",10,"儿科"]
[22,"G","儿童监护仪",1,"适用儿童患者的监护仪",2,"儿科",null,22]
[23,"G","电外科工作站",1,"自检系统、过载保护、功率智能控制系统、能量初始系统、脚踏开关无线远程控制等，可与超声刀等手术设备配套使用",32,"消化内科",null,20]
[24,"G","高频胸壁振荡排痰仪",1,"根据模拟正常生理咳嗽的原理，通过将患者所穿背心用管路连接到高速脉冲泵上，并快速地充气和放气，使患者胸壁发生有规律的舒张运动，患者气道和肺部发生自主的震颤气流和定向引流力，促使呼吸道粘液及各个肺叶深部代谢物松弛，液化、脱落；并在定向引流力的作用下将已液化脱落的代谢物按照选择的方向（如细支气管→支气管→气管）排出体外，",3,"呼吸内科"]
[25,"G","呼出一氧化氮测定系统",1,"可快速测定呼出气一氧化氮，可进行个性化的哮喘管理",6,"呼吸内科"]
[26,"B","多导睡眠监测",1,"主要用于诊断睡眠呼吸障碍，包括睡眠呼吸暂停综合症、鼾症、上气道阻力综合症，也用于其它睡眠障碍的辅助诊断，如：发作性睡病、不宁腿综合症、失眠分类等。包含：脑电（分析睡眠结构）、眼电、下颌肌电、口鼻气流和呼吸动度、心电、血氧、鼾声、肢动、体位等多个参数。",5,"呼吸内科"]
[27,"B","病床",30,"标准配置",7.5,"骨一"]
[28,"B","床头柜",30,"标准配置",3,"骨一"]
[29,"B","气垫床",3,"标准配置",0.20700000000000002,"骨一"]
[30,"B","输液架",3,"标准配置",0.06,"骨一"]
[31,"B","监护仪",3,"病房生理参数监护仪，部作品中",4.5,"心血管"]
[32,"G","气垫床",2,"标准配置",0.138,"心血管"]